[general]
bindport=4569
iaxcompat=yes
bandwidth=high
disallow=all
allow=all
allow=gsm                      ; Always allow GSM, it's cool :)
jitterbuffer=no
tos=lowdelay
context=trunkinbound

#include iax-vicidial.conf

